**RMD Telemetry Dictionary**

This document will serve to define and explain the format and syntax of all possible FSW commands to the Mini-NS.

Applicable Versions of the FSW:

|  |  |
| --- | --- |
| FSW Version | Applicable (Yes/No) |
| Version 1 | No |
| Version 2 | No |
| Version 3 | Yes |

[1. FSW Command Template 2](#_Toc3473956)

[2. Format Requirements 3](#_Toc3473957)

[3. Command Dictionary 4](#_Toc3473958)

[4. Appendix 8](#_Toc3473959)

[4.1 Byte-by-byte Breakdown of Mini-NS CCSDS Packet 8](#_Toc3473960)

[4.2 APID Table for Mini-NS CCSDS Packets 9](#_Toc3473961)

# FSW Command Template

**Function Name**

Description: A brief description of the command.

Syntax: This will give a general idea for the syntax of an FSW command. All fields will be specified and keywords/symbols for those fields are identified.

Example: An example of the syntax to use.

Command Length: The length of the command in bytes. Fields in the commands have fixed length. The length of a command includes the newline character which is used to terminate Mini-NS commands.

Field Format:

* A breakdown of each field listed in the command syntax. The data type (ie. INT, FLOAT, CHAR), the allowed range, as well as a description for that field are provided.
* Each command starts with a naming sequence, which is an ASCII character string
* Most commands include a detector number field, which allows commands to be sent to one of the two Mini-NS boards.

Byte Conversion: A conversion value to convert the ASCII command to a hex sequence for packing into a Payload Command Packet, RAW\_BYTES section.

Loop Status: Yes/no whether the system will begin a looping sequence after receiving this command.

Latency: The latency associated with this command. This number indicates the amount of time to wait before issuing any further commands.

Sub-commands: A list of commands which may be issued while this command is looping, if applicable.

Return Type: All Mini-NS return values come in the form of CCSDS packets. The APID of that packet indicates what type it is. Possible values are listed in this section.

Byte Breakdown: A description of all of the byte fields within the event or packet.

# Format Requirements

Commands are sent to the instrument as ASCII statements. Bytes received by the RS422 are interpreted as ASCII characters.

All commands have parameters which follow the command. Those parameters can be either integers, floats, or strings, as documented below. All parameters are required, and will be parsed as the expected data type. Any input given to the command will be parsed as the data type given. If the number of parameters is too few or too many, the command will be rejected with a Command Failure packet (0x01).

* **The parsing relies on the “\_” (underscore) character.**

Parameters and naming sequences not separated by the underscore will not be recognized by the system.

The number which follows almost all the commands is the Detector ID (0 or 1) indicated as “#” (pound) in the command list below. The Mini-NS is comprised of two separate boards and commands need to be addressed to one or the other board.

Each board will parse, but silently reject commands which are addressed to the other board.

* **Commands must be terminated with a newline “\n” character.**

On the completion of a command, the return value will be written to the RS422 wrapped in a CCSDS packet; these return values are listed below each command. The success or failure of a command is indicated via the APID bytes (ie. the type of packet returned), see the appendix. All commanded functions return a CCSDS packet upon completion, but some output a packet other than SUCCESS if successful (eg. GETSTAT returns an SOH packet instead of a SUCCESS packet).

# Command Dictionary

## Get Status (NO-OP)

Description: Request the Statement of Health information of the instrument. The Mini-NS will output a single SOH packet.

Syntax: MNS\_GETSTAT\_#

Example: MNS\_GETSTAT\_0\n

Command Length: 14 bytes

Field Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Format | Description | Data Type | Value Range |
| MNS\_GETSTAT | Naming Sequence | ASCII string | - |
| # | Detector Number | Integer | 0, 1 |

Byte Conversion: N/A

Loop Status: No

Latency: N/A

Sub-commands: None

Return Type: Statement of Health (0x22)

Byte Breakdown: Table 2 lays out the bytes for the first packet only for the Level 3 FSW currently on the RMD engineering board (3-15-2019).

The value of byte 4 depends on the CCSDS flags and the detector number:

* Detector 0 = 0x0A
* Detector 1 = 0x0B

The value for byte 5 is the APID which is 0x22 for SOH packets.

The value for byte 6 will always be 0xC0, as SOH packets are always unsegmented (group flags) and the sequence count is always 1, leaving the MSB for sequence count zeroes. The value for byte 7 will always be 0x01.

The packet length (byte 8, 9) will always be 29 for SOH packets so byte 8 is always 0x00 and byte 9 is always 0x1D.

The fields within an SOH packet are comprised of the current temperature of each temperature sensor within the detector; each detector has a temperature sensor on the digital board, on the analog board, and on one module. The temperature is reported as a signed 4-byte wide field.

Aggregated neutrons is a signed 4-byte wide field which reports the aggregated total neutron counts over a science run. This number will be incrementing during DAQ mode, but static all other times.

Local time is a signed 4-byte wide field which reports the processor time and should always be incrementing at 1 Hz. Depending on how busy the processor, this may skip a second from time-to-time.




Figure 1: Checksum Calculation

To calculate the RMD checksums (2 8-bit checksums), we iterate over the secondary CCSDS header and the payload data bytes and calculate a simple and Fletcher checksum. To find the BCT checksum (1 16-bit checksum), we add the byte values from byte 5 through the RMD checksums together.

Table 1: RMD General Statement of Health Format

|  |  |  |
| --- | --- | --- |
| Byte | Description | Group |
| 0-3 | Sync Marker | Primary CCSDS Header |
| 4 | Flags and Detector Number: |
| 5 | APID |
| 6 | Group Flags and Sequence Count MSB |
| 7 | Sequence Count LSB |
| 8 | Packet Length MSB |
| 9 | Packet Length LSB |
| 10 | Reset Request Flag | Secondary CCSDS Header |
| 11-14 | Analog Board Temp. | Data |
| 15 | “\t” |
| 16-19 | Digital Board Temp. |
| 20 | “\t” |
| 21-24 | Module Temp. Sensor |
| 25 | “\t” |
| 26-29 | Agg. Neutrons w/PSD |
| 30 | “\t” |
| 31-34 | Local Time |
| 35 | “\n” |
| 36 | Simple Checksum | RMD Data Checksums |
| 37 | Fletcher Checksum |
| 38 | CCSDS Checksum MSB | Checksum |
| 39 | CCSDS Checksum LSB |

Table 2: Values for an SOH Packet

|  |  |  |
| --- | --- | --- |
| Byte | Description | Group |
| 0 | 0x35 | Sync Marker |
| 1 | 0x2E |
| 2 | 0xF8 |
| 3 | 0x53 |
| 4 | 0x0A | Primary CCSDS Header |
| 5 | 0x22 |
| 6 | 0xC0 |
| 7 | 0x01 |
| 8 | 0x00 |
| 9 | 0x1D |
| 10 | 0x00 | Secondary CCSDS Header |
| 11-14 | Byte 11 = 0x00  Byte 12 = 0x00  Byte 13 = 0x00  Byte 14 = 0x19 | Mini-NS Data Bytes |
| 15 | 0x09 |
| 16-19 | Byte 16 = 0x00  Byte 17 = 0x00  Byte 18 = 0x00  Byte 19 = 0x01 |
| 20 | 0x09 |
| 21-24 | Byte 21 = 0x00  Byte 22 = 0x00  Byte 23 = 0x00  Byte 24 = 0x19 |
| 25 | 0x09 |
| 26-29 | Byte 26 = 0x00  Byte 27 = 0x00  Byte 28 = 0x00  Byte 29 = 0x32 |
| 30 | 0x09 |
| 31-34 | Byte 31 = 0x00  Byte 32 = 0x00  Byte 33 = 0x00  Byte 34 = 0x02 |
| 35 | 0x0A |
| 36 | 0x09 | RMD Simple Checksum |
| 37 | 0x5D | RMD Fletcher Checksum |
| 38 | 0x03 | CCSDS Checksum MSB |
| 39 | 0x06 | CCSDS Checksum LSB |

## Initialize Data Acquisition Run

Description: Initialize the system and prepare to take science data. The active components are energized, data objects are created in the code, and parameters for operation are loaded (e.g. HV is set). Data files are generated and opened. The system will be in a new polling loop.

Syntax: MNS\_DAQ\_#\_IDNumber

Example: MNS\_DAQ\_0\_000001\n

Command Length: 17 bytes

Field Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Format | Description | Data Type | Value Range |
| MNS\_DAQ | Naming Sequence | ASCII string | - |
| # | Detector Number | Integer | 0, 1 |
| ID Number | Unique Run Number | Integer | 0 - 999999 |

Byte Conversion: N/A

Loop Status: Yes

Latency: N/A

Sub-commands: MNS\_START, MNS\_END, MNS\_BREAK, MNS\_READTEMP

Return Type: Command Success (0x00), Command Failure (0x01)

# Data Product Packet Type Dictionary

## Event-by-event Data Product (EVT)

Description: The full context of a data acquisition run.

How to Acquire: MNS\_TX command

Packet Length: 2037 bytes

Field Format:

|  |  |  |  |
| --- | --- | --- | --- |
| Format | Description | Data Type | Value Range |
| MNS\_TX | Naming Sequence | ASCII string | - |
| # | Detector Number | Integer | 0, 1 |
| Type | Data Product Type | Integer | 0-8 |
| IDNum | DAQ ID Number | Integer | 0-9999 |
| RunNum | DAQ Run Number | Integer | 0-9999 |
| SetNum | DAQ Set Number | Integer | 0-75 (estimated) |

Byte Conversion: N/A

Return Type: 0x77

Byte Breakdown: This data product is characterized by having a CCSDS header, a secondary header, a data header, data bytes, and checksums.

|  |  |  |  |
| --- | --- | --- | --- |
| Section | Description | Length (bytes) | Grouping |
| CCSDS Header | Header for acceptance by XB-1 | 10 | CCSDS Header |
| Secondary CCSDS Header | Reset Request Bytes | 1 | Data Bytes |
| RMD Data Header | System configuration parameters | 70 | Data Bytes |
| Data Bytes | Data product events | 1952 | Data Bytes |
| RMD Checksums | Simple, Fletcher | 2 | Data Bytes |
| Checksums | Checksums for XB-1 | 2 | Checksums |

# Appendix

## Byte-by-byte Breakdown of Mini-NS CCSDS Packet

|  |  |  |
| --- | --- | --- |
| Byte | Description | Group |
| 0 | 0x35 | Sync Marker |
| 1 | 0x2E |
| 2 | 0xF8 |
| 3 | 0x53 |
| 4 | 7:5 - CCSDS Version Number = 000  4 - Packet Type (P.T.) = 0  3 - Secondary Header Flag (S.H.) = 1  2:0 – APID MSB = 010 for Mini-NS Detector 0  = 011 for Mini-NS Detector 1  0x0A = Detector 0  0x0B = Detector 1 | Primary CCSDS Header |
| 5 | APID LSB = 0x00 – 0xFF |
| 6 | 7:6 – Group Flags = 00 for intermediate packet  = 01 for first packet  = 10 for last packet  = 11 for unsegmented packet  5:0 – Sequence Count MSB |
| 7 | Sequence Count LSB |
| 8 | Packet Length MSB |
| 9 | Packet Length LSB |
| 10 | Reset Request = 0x00 – No request for reset  = 0x0F – Power off the detector  = 0xFF – Power cycle the detector to STDBY  = 0xF0 – Power cycle the detector to DAQ | Secondary CCSDS Header |
| 11 | Payload Data Byte 0 | Mini-NS Data Bytes |
| … | Payload Data Byte 2026 (max N = 2026) |
| N-1 | Simple Checksum | RMD Data Checksums |
| N | Fletcher Checksum |
| N+1 | Checksum MSB | Checksums |
| N+2 | Checksum LSB |

## APID Table for Mini-NS CCSDS Packets

|  |  |  |
| --- | --- | --- |
| APID LSB | Value | Description |
| Command Success | 0x00 | The input command was successfully executed |
| Command Failure | 0x11 | The input command failed somewhere during execution |
| Statement of Health | 0x22 | Packet contains statement of health information |
| LS Files Return | 0x33 | Packet contains filenames and file sizes for all the file on the Mini-NS SD card |
| Temperature | 0x44 | Packet with the most current temperatures. |
| MNS\_CPS | 0x55 | Neutron Counts per Second Data |
| MNS\_WAV | 0x66 | Waveform Data |
| MNS\_EVTS | 0x77 | Event by Event Data |
| MNS\_2DH | 0x88 | 2D Histogram Data |
| Log File | 0x99 | Log File |
| Configuration File | 0xAA | Configuration File |